## /score/mesh/rotate/

Mesh rotation commands.

## Sub-directories :

## Commands :

reset

  Reset rotation angles of the scoring mesh.

  Available at all Geant4 states.

rotateX [Rx] [Unit]

  Rotate the scoring mesh in X axis.

  Available at all Geant4 states.

  Parameters

  Rx | type d |  |
  Unit | type s | Omittable : default value = deg | Parameter candidates : rad mrad sr deg radian milliradian steradian degree

rotateY [Ry] [Unit]

  Rotate the scoring mesh in Y axis.

  Available at all Geant4 states.

  Parameters

  Ry | type d |  |
  Unit | type s | Omittable : default value = deg | Parameter candidates : rad mrad sr deg radian milliradian steradian degree

rotateZ [Rz] [Unit]

  Rotate the scoring mesh in Z axis.

  Available at all Geant4 states.

  Parameters

  Rz | type d |  |
  Unit | type s | Omittable : default value = deg | Parameter candidates : rad mrad sr deg radian milliradian steradian degree