## /vis/modeling/trajectories/drawByParticleID-0/

Commands for drawByParticleID-0 model.

## Sub-directories :

/vis/modeling/trajectories/drawByParticleID-0/default/

  Commands for default configuration

## Commands :

set [Variable] [Value]

  Set variable colour through a string

  Available at all Geant4 states.

  Parameters

  Variable | type s |  |
  Value | type s |  |

setRGBA [Variable] [Red component] [Green component] [Blue component] [Alpha component]

  Set variable colour through red, green, blue and alpha components

  Available at all Geant4 states.

  Parameters

  Variable | type s |  |
  Red component | type d |  |
  Green component | type d |  |
  Blue component | type d |  |
  Alpha component | type d |  |

setDefault [Variable]

  Set colour through a string

  Available at all Geant4 states.

  Parameters

  Variable | type s |  |

setDefaultRGBA [Red component] [Green component] [Blue component] [Alpha component]

  Set colour through red, green, blue and alpha components
  Four inputs are expected.

  Available at all Geant4 states.

  Parameters

  Red component | type d |  |
  Green component | type d |  |
  Blue component | type d |  |
  Alpha component | type d |  |

verbose [Bool]

  Verbose command

  Available at all Geant4 states.

  Parameters

  Bool | type b |  |