
        ############################################
        !!! WARNING - FPE detection is activated !!!
        ############################################

*************************************************************
 Geant4 version Name: geant4-09-03-ref-06    (25-June-2010)
                      Copyright : Geant4 Collaboration
                      Reference : NIM A 506 (2003), 250-303
                            WWW : http://cern.ch/geant4
*************************************************************


***** Table : Nb of materials = 14 *****

 Material:      Air     density:  1.290 mg/cm3  RadL: 285.161 m    Nucl.Int.Length: 662.680 m    Imean:  85.703 eV   temperature: 273.15 K  pressure:   1.00 atm
   --->  Element: Nitrogen (N)   Z =  7.0   N =  14.0   A =  14.01 g/mole  ElmMassFraction:  70.00 %  ElmAbundance  72.71 %
   --->  Element: Oxygen (O)   Z =  8.0   N =  16.0   A =  16.00 g/mole  ElmMassFraction:  30.00 %  ElmAbundance  27.29 %

 Material: H2liquid     density: 70.800 mg/cm3  RadL:   8.923 m    Nucl.Int.Length:   4.960 m    Imean:  19.200 eV 
   --->  Element: Hydrogen (H)   Z =  1.0   N =   1.0   A =   1.01 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material:    Water     density:  1.000 g/cm3   RadL:  36.092 cm   Nucl.Int.Length:  75.416 cm   Imean:  75.000 eV 
   --->  Element: Hydrogen (H)   Z =  1.0   N =   1.0   A =   1.01 g/mole  ElmMassFraction:  11.21 %  ElmAbundance  66.67 %
   --->  Element: Oxygen (O)   Z =  8.0   N =  16.0   A =  16.00 g/mole  ElmMassFraction:  88.79 %  ElmAbundance  33.33 %

 Material:      CO2     density:  0.001 kg/m3   RadL: 361.873 km   Nucl.Int.Length: 858.384 km   Imean:  90.958 eV   temperature: 273.15 K  pressure:   1.00 atm
   --->  Element: Hydrogen (C)   Z =  6.0   N =  12.0   A =  12.00 g/mole  ElmMassFraction:  27.27 %  ElmAbundance  33.33 %
   --->  Element: Oxygen (O)   Z =  8.0   N =  16.0   A =  16.00 g/mole  ElmMassFraction:  72.73 %  ElmAbundance  66.67 %

 Material:   D2_gas     density:  0.036 kg/m3   RadL:  13.184 km   Nucl.Int.Length:  12.278 km   Imean:  41.800 eV   temperature: 273.15 K  pressure:   1.00 atm
   --->  Element: D2_gas ( )   Z =  2.0   N =   2.0   A =   2.01 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material: liquidArgon     density:  1.390 g/cm3   RadL:  14.065 cm   Nucl.Int.Length:  86.078 cm   Imean: 188.000 eV 
   --->  Element: liquidArgon ( )   Z = 18.0   N =  40.0   A =  39.95 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material: Aluminium     density:  2.700 g/cm3   RadL:   8.893 cm   Nucl.Int.Length:  38.879 cm   Imean: 166.000 eV 
   --->  Element: Aluminium ( )   Z = 13.0   N =  27.0   A =  26.98 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material:  Silicon     density:  2.330 g/cm3   RadL:   9.368 cm   Nucl.Int.Length:  45.663 cm   Imean: 173.000 eV 
   --->  Element: Silicon ( )   Z = 14.0   N =  28.1   A =  28.09 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material: Germanium     density:  5.323 g/cm3   RadL:   2.301 cm   Nucl.Int.Length:  27.431 cm   Imean: 350.000 eV 
   --->  Element: Germanium ( )   Z = 32.0   N =  72.6   A =  72.61 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material:      BGO     density:  7.100 g/cm3   RadL:   1.123 cm   Nucl.Int.Length:  22.806 cm   Imean: 473.785 eV 
   --->  Element: Oxygen (O)   Z =  8.0   N =  16.0   A =  16.00 g/mole  ElmMassFraction:  15.41 %  ElmAbundance  63.16 %
   --->  Element: Germanium (Ge)   Z = 32.0   N =  72.6   A =  72.59 g/mole  ElmMassFraction:  17.48 %  ElmAbundance  15.79 %
   --->  Element: Bismuth (Bi)   Z = 83.0   N = 209.0   A = 208.98 g/mole  ElmMassFraction:  67.10 %  ElmAbundance  21.05 %

 Material:     Iron     density:  7.870 g/cm3   RadL:   1.759 cm   Nucl.Int.Length:  16.999 cm   Imean: 286.000 eV 
   --->  Element: Iron ( )   Z = 26.0   N =  55.8   A =  55.85 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material: Tungsten     density: 19.300 g/cm3   RadL:   3.504 mm   Nucl.Int.Length:  10.312 cm   Imean: 727.000 eV 
   --->  Element: Tungsten ( )   Z = 74.0   N = 183.8   A = 183.85 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material:     Lead     density: 11.350 g/cm3   RadL:   5.612 mm   Nucl.Int.Length:  18.247 cm   Imean: 823.000 eV 
   --->  Element: Lead ( )   Z = 82.0   N = 207.2   A = 207.19 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %

 Material:  Uranium     density: 18.950 g/cm3   RadL:   3.166 mm   Nucl.Int.Length:  11.446 cm   Imean: 890.000 eV 
   --->  Element: Uranium ( )   Z = 92.0   N = 238.0   A = 238.03 g/mole  ElmMassFraction: 100.00 %  ElmAbundance 100.00 %


/run/verbose 2
#
/testem/det/setMat Aluminium
/testem/det/setSize 10 m
#
/run/initialize
userDetector->Construct() start.

 The Box is 10 m   of Aluminium
Aluminium is registered to the default region.
physicsList->Construct() start.
physicsList->Construct() start.
physicsList->CheckParticleList() start.
physicsList->setCut() start.
PhysicsList::SetCuts:CutLength : 1 mm 
#
/testem/gun/setDefault
/gun/particle e-
/gun/energy 100 MeV
#
/testem/histo/setHisto 1 100 0 50 cm
----> SetHisto 1: total track length of primary particle (cm);  100 bins from 0 cm to 50 cm
/testem/histo/setHisto 2 100 0 300 none
----> SetHisto 2: nb steps of primary particle;  100 bins from 0 none to 300 none
/testem/histo/setHisto 3 200 0 20 mm
----> SetHisto 3: step size of primary particle (mm);  200 bins from 0 mm to 20 mm
#
/testem/histo/setFileType root
#
/testem/phys/setCuts 1 mm
/testem/histo/setFileName run0
/run/beamOn 2000

phot:   for  gamma    SubType= 12
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
       PhotoElectric :     Emin=          0 eV         Emax=   100 TeV

compt:   for  gamma    SubType= 13
      Lambda tables from 100 eV  to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
       Klein-Nishina :     Emin=          0 eV         Emax=   100 TeV

conv:   for  gamma    SubType= 14
      Lambda tables from 1.022 MeV to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
       Bethe-Heitler :     Emin=          0 eV         Emax=   100 TeV

msc:   for e-    SubType= 10
      Lambda tables from 100 eV  to 100 TeV in 240 bins, spline: 1
      RangeFactor= 0.04, stepLimitType: 2, latDisplacement: 1, skin= 3, geomFactor= 2.5
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
          UrbanMsc93 :     Emin=          0 eV         Emax=   100 TeV

eIoni:   for  e-    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
        MollerBhabha :     Emin=          0 eV         Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

eBrem:   for  e-    SubType= 3
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      LPM flag: 1 for E > 1 GeV
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               eBrem :     Emin=          0 eV         Emax=   1 GeV
            eBremRel :     Emin=          1 GeV        Emax=   100 TeV

eIoni:   for  e+    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
        MollerBhabha :     Emin=          0 eV         Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

eBrem:   for  e+    SubType= 3
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      LPM flag: 1 for E > 1 GeV
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               eBrem :     Emin=          0 eV         Emax=   1 GeV
            eBremRel :     Emin=          1 GeV        Emax=   100 TeV

annihil:   for  e+    SubType= 5
      Lambda tables from 100 eV  to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
            eplus2gg :     Emin=          0 eV         Emax=   100 TeV

msc:   for proton    SubType= 10
      Lambda tables from 100 eV  to 100 TeV in 240 bins, spline: 1
      RangeFactor= 0.04, stepLimitType: 2, latDisplacement: 1, skin= 3, geomFactor= 2.5
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
          UrbanMsc90 :     Emin=          0 eV         Emax=   100 TeV

hIoni:   for  proton    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               Bragg :     Emin=          0 eV         Emax=   2 MeV
          BetheBloch :     Emin=          2 MeV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

hBrems:   for  proton    SubType= 3
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               hBrem :     Emin=          0 eV         Emax=   100 TeV

hPairProd:   for  proton    SubType= 4
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
           hPairProd :     Emin=          0 eV         Emax=   100 TeV

msc:   for GenericIon    SubType= 10
      RangeFactor= 0.2, stepLimitType: 0, latDisplacement: 0
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
          UrbanMsc90 :     Emin=          0 eV         Emax=   100 TeV

ionIoni:   for  GenericIon    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      Stopping Power data for 17 ion/material pairs, nuclearStopping: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
            BraggIon :     Emin=          0 eV         Emax=   2 MeV
          BetheBloch :     Emin=          2 MeV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

hIoni:   for  anti_proton    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
            ICRU73QO :     Emin=          0 eV         Emax=   2 MeV
          BetheBloch :     Emin=          2 MeV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

hIoni:   for  kaon+    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               Bragg :     Emin=          0 eV         Emax=   1.05231 MeV
          BetheBloch :     Emin=    1.05231 MeV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

hIoni:   for  kaon-    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
            ICRU73QO :     Emin=          0 eV         Emax=   1.05231 MeV
          BetheBloch :     Emin=    1.05231 MeV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

muMsc:   for mu+    SubType= 10
      Lambda tables from 100 eV  to 100 TeV in 240 bins, spline: 1
      RangeFactor= 0.04, step limit type: 2, lateralDisplacement: 1, polarAngleLimit(deg)= 0
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
          UrbanMsc90 :     Emin=          0 eV         Emax=   100 TeV

muIoni:   for  mu+    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               Bragg :     Emin=          0 eV         Emax=   200 keV
          BetheBloch :     Emin=        200 keV        Emax=   1 GeV
        MuBetheBloch :     Emin=          1 GeV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

muBrems:   for  mu+    SubType= 3
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
              MuBrem :     Emin=          0 eV         Emax=   100 TeV

muPairProd:   for  mu+    SubType= 4
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
          muPairProd :     Emin=          0 eV         Emax=   100 TeV

muIoni:   for  mu-    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
            ICRU73QO :     Emin=          0 eV         Emax=   200 keV
          BetheBloch :     Emin=        200 keV        Emax=   1 GeV
        MuBetheBloch :     Emin=          1 GeV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

muBrems:   for  mu-    SubType= 3
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
              MuBrem :     Emin=          0 eV         Emax=   100 TeV

muPairProd:   for  mu-    SubType= 4
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
          muPairProd :     Emin=          0 eV         Emax=   100 TeV

hIoni:   for  pi+    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               Bragg :     Emin=          0 eV         Emax=   297.504 keV
          BetheBloch :     Emin=    297.504 keV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

hBrems:   for  pi+    SubType= 3
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               hBrem :     Emin=          0 eV         Emax=   100 TeV

hPairProd:   for  pi+    SubType= 4
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
           hPairProd :     Emin=          0 eV         Emax=   100 TeV

msc:   for pi-    SubType= 10
      Lambda tables from 100 eV  to 100 TeV in 240 bins, spline: 1
      RangeFactor= 0.04, stepLimitType: 2, latDisplacement: 1, skin= 3, geomFactor= 2.5
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
          UrbanMsc90 :     Emin=          0 eV         Emax=   100 TeV

hIoni:   for  pi-    SubType= 2
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      finalRange(mm)= 0.1, dRoverRange= 0.2, integral: 1, fluct: 1, linLossLimit= 0.01
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
            ICRU73QO :     Emin=          0 eV         Emax=   297.504 keV
          BetheBloch :     Emin=    297.504 keV        Emax=   100 TeV
      CSDA range table up to 1 GeV in 160 bins

hBrems:   for  pi-    SubType= 3
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
               hBrem :     Emin=          0 eV         Emax=   100 TeV

hPairProd:   for  pi-    SubType= 4
      dE/dx and range tables from 100 eV  to 100 TeV in 240 bins
      Lambda tables from threshold to 100 TeV in 240 bins, spline: 1
      ===== EM models for the G4Region  DefaultRegionForTheWorld ======
           hPairProd :     Emin=          0 eV         Emax=   100 TeV

Region <DefaultRegionForTheWorld> -- appears in <Aluminium> world volume
 Root logical volume(s) : Aluminium 
 Pointers : G4VUserRegionInformation[0], G4UserLimits[0], G4FastSimulationManager[0], G4UserSteppingAction[0]
 Materials : Aluminium 
 Production cuts :   gamma 1 mm      e- 1 mm      e+ 1 mm  proton 0 fm 

========= Table of registered couples ==============================

Index : 0     used in the geometry : Yes     recalculation needed : No 
 Material : Aluminium
 Range cuts        :  gamma  1 mm     e-  1 mm     e+  1 mm  proton 0 fm 
 Energy thresholds :  gamma  6.90363 keV    e-  598.345 keV    e+  570.85 keV proton 0 eV 
 Region(s) which use this couple : 
    DefaultRegionForTheWorld

====================================================================

Start closing geometry.
G4GeometryManager::ReportVoxelStats -- Voxel Statistics

    Total memory consumed for geometry optimisation:   0 kByte
    Total CPU time elapsed for geometry optimisation: 0 seconds
### Run 0 start.

--------- Ranecu engine status ---------
 Initial seed (index) = 0
 Current couple of seeds = 9876, 54321
----------------------------------------
Start Run processing.

---> Begin of Event: 0
Run terminated.
Run Summary
  Number of events processed : 2000
  User=7.79s Real=10.03s Sys=0.06s

 ======================== run summary ======================

 The run was: 2000 e- of 100 MeV through 10 m   of Aluminium (density: 2.7 g/cm3 )

 ============================================================

 total energy deposit: 99.805 MeV

 nb tracks/event   neutral:     27.763   charged:     147.75
 nb  steps/event   neutral:     140.71   charged:     474.47

 nb of process calls per event: 
   Transportation     annihil       compt        conv       eBrem       eIoni         msc        phot
         0.9535      1.4375      112.95      1.4375      25.132      299.93      147.97      25.375

---------------------------------------------------------
 Primary particle : 
 true Range = 10.943 cm    rms = 3.7796 cm 
 proj Range = 9.5296 cm    rms = 3.5049 cm 
 proj/true  = 0.87081
 transverse dispersion at end = 1.6774 cm 
      mass true Range from simulation = 29.547 g/cm2 
       from PhysicsTable (csda range) = 31.721 g/cm2 
---------------------------------------------------------


--------- Ranecu engine status ---------
 Initial seed (index) = 0
 Current couple of seeds = 1106853113, 1573199675
----------------------------------------
#
/process/eLoss/verbose 0
#
/testem/phys/setCuts 10 um
/testem/histo/setFileName run1
/run/beamOn 2000

Region <DefaultRegionForTheWorld> -- appears in <Aluminium> world volume
 Root logical volume(s) : Aluminium 
 Pointers : G4VUserRegionInformation[0], G4UserLimits[0], G4FastSimulationManager[0], G4UserSteppingAction[0]
 Materials : Aluminium 
 Production cuts :   gamma 10 um      e- 10 um      e+ 10 um  proton 0 fm 

========= Table of registered couples ==============================

Index : 0     used in the geometry : Yes     recalculation needed : No 
 Material : Aluminium
 Range cuts        :  gamma  10 um     e-  10 um     e+  10 um  proton 0 fm 
 Energy thresholds :  gamma  990 eV     e-  34.172517 keV    e+  33.943645 keV proton 0 eV 
 Region(s) which use this couple : 
    DefaultRegionForTheWorld

====================================================================

### Run 1 start.

--------- Ranecu engine status ---------
 Initial seed (index) = 0
 Current couple of seeds = 1106853113, 1573199675
----------------------------------------
Start Run processing.

---> Begin of Event: 0
Run terminated.
Run Summary
  Number of events processed : 2000
  User=14.77s Real=18.99s Sys=0.06s

 ======================== run summary ======================

 The run was: 2000 e- of 100 MeV through 10 m   of Aluminium (density: 2.7 g/cm3 )

 ============================================================

 total energy deposit: 99.801 MeV

 nb tracks/event   neutral:     34.728   charged:     287.34
 nb  steps/event   neutral:     144.43   charged:      893.9

 nb of process calls per event: 
   Transportation     annihil       compt        conv       eBrem       eIoni         msc        phot
          0.985      1.3815       109.7      1.3815      32.861       577.2      282.45      32.369

---------------------------------------------------------
 Primary particle : 
 true Range = 11.119 cm    rms = 3.7672 cm 
 proj Range = 9.6327 cm    rms = 3.4858 cm 
 proj/true  = 0.86636
 transverse dispersion at end = 1.7471 cm 
      mass true Range from simulation = 30.02 g/cm2 
       from PhysicsTable (csda range) = 31.721 g/cm2 
---------------------------------------------------------


--------- Ranecu engine status ---------
 Initial seed (index) = 0
 Current couple of seeds = 1339043857, 385085779
----------------------------------------
UserDetectorConstruction deleted.
UserPhysicsList deleted.
UserRunAction deleted.
UserPrimaryGenerator deleted.
G4 kernel has come to Quit state.
EventManager deleted.
UImanager deleted.
Units table cleared.
StateManager deleted.
RunManagerKernel is deleted.
RunManager is deleting.

